When using the Notepad, to wrap text to the window size, click on Word Wrap from Format or Edit menu of the Notepad.
Notes: A check mark will appear when word wrap is turned on.
Wrapping text enables you to see all the text on the line, but it doesn't affect the way text appears when it is printed.

=========================================================================
ReadMe File for TWAIN Driver's Software for Type1/Type2/Type3/Type4/Type5
=========================================================================

It is our pleasure to introduce TWAIN Driver Software for Type1/Type2/Type3/Type4/Type5 units.
Please read the following instructions for the software before installation.

Note: "Type1" means MFX-1200/1250/1300, "Type2" means MFX-1600/1700, "Type3" means MFX-2500/2530, "Type4" means F-360, and "Type5" means F-320.


************************************************************
CONTENTS
************************************************************

I.   READ BEFORE INSTALLATION
      SOFTWARE LICENSE

II.  PRODUCT INTRODUCTION
      PURPOSE OF THIS README FILE
      WHO NEEDS THIS SOFTWARE?
      SOFTWARE COMPONENTS

III. INSTALLATION/UNINSTALLATION INSTRUCTION
      INSTALLATION INSTRUCTION
      UNINSTALLER/UNINSTALLATION INSTRUCTION

IV.  HINTS
      BI-DIRECTIONAL PARALLEL INTERFACE
      "CAN NOT WRITE TO LPT1"/"TRANSFERRING DATA ERROR"/"THERE IS NO RESPONSE FROM DEVICE"
      LIMITATION OF ENLARGEMENT FUNCTION
      FOR THE USERS OF WINDOWS NT 4.0
      FOR THE USERS OF WINDOWS 2000
      FOR THE USERS OF MICROSOFT OFFICE 2000(WORD/EXCEL/POWERPOINT)
      FOR THE USERS OF CAERE OMNIPAGE PRO 10.0
      FOR THE USERS OF SCANSOFT TEXTBRIDGE PRO MILLENNIUM VER.9.5
      FOR THE USERS OF SCANSOFT PAPERPORT DELUXE 6.5/7.0
      FOR USERS OF I.R.I.S READIRIS PRO 6

V.   TRADEMARK NOTICES


************************************************************
I. READ BEFORE INSTALLATION
************************************************************

------------------------------------------------------------
SOFTWARE LICENSE
------------------------------------------------------------

1. Any and all copyright and any other intellectual property regarding the Software remain solely the property of Destiny Technology Corporation (hereinafter "Destiny") and MURATA MACHINERY,LTD. (hereinafter "Murata").

2. You may use the Software only in the country of your purchase and only for the purpose of using the hardware of Murata and other companies approved by Murata (hereinafter "OEM Companies").

3. You may use the Software only in compliance with notices and restrictions written in "Installation Manual" and other documents contained in this package.

4. You must not modify, alter all or any part of the Software. You must not make any attempt to discover the source code of the Software by any method including reverse-engineering, de-compiling, or de-assembling.

5. You must not sell, transfer, rent, lease or sublicense the Software to any third party by transmitting the software via phone-line or network, or by copying the software to floppy disk, CD-ROM, magnetic data tape or any other media.

6. The software is subject to changes by Murata or Destiny in its specifications and program without any prior notice.

7. Before installing the software, you are supposed to take any and all procedures necessary to secure your records and data at your cost and responsibility, including making backup of your computer files. Neither Murata, Destiny, OEM Companies nor their distributors/sub-distributors shall be liable for any damage or loss caused by your failure of taking the foregoing procedure.

8. Neither Murata, Destiny, OEM Companies nor their distributors/sub-distributors shall be liable for any damage or loss caused by (1) use of the software in combination with the hardware other than the hardware which is defined in Section 2 above or (2) modification of the software.

9. Neither Murata, Destiny, OEM Companies nor their distributors/sub-distributors shall assume any damages incurred by you or a third party even if such damage is directly/indirectly caused by use of the software or incapability to use the software.


************************************************************
II. PRODUCT INTRODUCTION
************************************************************

------------------------------------------------------------
PURPOSE OF THIS README FILE
------------------------------------------------------------

This ReadMe file provides specific installation instructions, precautions, restrictions and other information of TWAIN Driver's Software for Type1/Type2/Type3/Type4/Type5 before you install and use them. Installation instructions are provided for the following operating systems:

	* Windows Vista(R)
	* Windows(R) XP
	* Windows(R) 2000
	* Windows NT(R) 4.0
	* Windows(R) Me
	* Windows(R) 98 SE
	* Windows(R) 98
	* Windows(R) 95

The scanner driver does not support Windows Server(R) 2008.

For the detailed information, refer to the on-line help included in each software component.

------------------------------------------------------------
WHO NEEDS THIS SOFTWARE?
------------------------------------------------------------

This TWAIN Driver's Software enables scanning images with Type1/Type2/Type3/Type4/Type5 units.

-----------------------
SOFTWARE COMPONENTS
-----------------------

This software consists of a TWAIN Driver.

Using this TWAIN Driver, applications supporting TWAIN, such as "Photoshop" and "Imaging", can retrieve the scanned data from Type1/Type2/Type3/Type4/Type5.


************************************************************
III. INSTALLATION/UNINSTALLATION INSTRUCTION
************************************************************

The software has 4 installers (for Windows 95/98/Me, for Windows NT 4.0/2000, for Windows XP, for Windows Vista). Please use the correct installer. You can install the software using the Setup.exe file. 

------------------------------------------------------------
INSTALLATION INSTRUCTION
------------------------------------------------------------

Administrator privileges are required to install the software onto a Windows NT 4.0 system, a Windows 2000 system, a Windows XP system and a Windows Vista system.

Installation from Setup.exe

Use the installation CD-ROM (TWAIN Driver's Setup Disc). Network clients can install it from the network directory, in which the contents of the CD-ROM are copied.

1. Close all applications. Turn off virus checkers and Terminate Stay Resident (TSR) programs. After installation, these programs can be turned back on.
2. Insert the CD-ROM (Windows 95/98/Me users may also go to network drive location as assigned by Network Administrator).
3. Select "Run" from the Start menu on your task-bar.
4. Browse to the Setup directory on the CD-ROM drive (or Windows 95/98/Me users may go to a network directory location as assigned by the Network Administrator).
5. Select the "Setup.exe" file; click "OK".
6. Follow the prompts.

------------------------------------------------------------
UNINSTALLER/UNINSTALLATION INSTRUCTION
------------------------------------------------------------

This software does not contain Uninstaller. User can uninstall it from the Control Panel.

Starting the Uninstaller

Administrator privileges are required to uninstall the software from a Windows NT 4.0 system, a Windows 2000 system, a Windows XP system and a Windows Vista system.

1. Select "Setting" from the Start menu on your task-bar and select "Control Panel" from the submenu. (In Windows XP and Windows Vista, select "Control Panel" from the Start menu.)
   On the Control Panel, click "Add/Remove Programs". (In Windows Vista, click "Uninstall a Program")
2. On the "Add/Remove Programs" Dialog, select "TWAIN Driver" from the middle list.
3. Click "Add/Remove" Button.
4. Click "Yes" on the following "Confirm File Deletion" Dialog.
5. Follow the prompts.


******************************************************
IV. HINTS
******************************************************

------------------------------------------------------------
BI-DIRECTIONAL PARALLEL INTERFACE
------------------------------------------------------------

This TWAIN driver supports the Nibble mode and the ECP mode for the bi-directional parallel interface. As the speed of data transferring with the ECP mode is faster than the Nibble mode, we recommend use of a PC that supports the ECP mode.

------------------------------------------------------------
"CAN NOT WRITE TO LPT1"/"TRANSFERRING DATA ERROR"/"THERE IS NO RESPONSE FROM DEVICE"
------------------------------------------------------------

If you encounter these problems, please try the following.

   1. Scanning and Data Transferring can not be executed during PC printing. In this case, perform them after finishing printing.
   2. If your PC printer port is set to the ECP mode, change to the Nibble mode (only in Windows 95/98/Me).
   3. If you are using a long cable (more than 3m), change to a shorter cable (less than 3m).

------------------------------------------------------------
LIMITATION OF ENLARGEMENT FUNCTION
------------------------------------------------------------

If your machine is Type1 or Type2, the enlargement scan function is not available when you use the ADF. 
Also, if your machine is Type2, it is not available when you set the resolution to 600 dpi. 
And, if your machine is Type4 or Type5, the enlargement scan function is not available.

------------------------------------------------------------
FOR THE USERS OF WINDOWS NT 4.0
------------------------------------------------------------

1. You cannot use this TWAIN driver with "Imaging" software, which is included in Windows NT 4.0, because it does not support TWAIN.
2. Windows NT 4.0 does not support the ECP mode for the bi-directional parallel interface. Therefore the data will be transferred with the Nibble mode.

------------------------------------------------------------
FOR THE USERS OF WINDOWS 2000
------------------------------------------------------------

Windows 2000 does not support the ECP mode for the bi-directional parallel interface. Therefore the data will be transferred with the Nibble mode.

------------------------------------------------------------
FOR THE USERS OF MICROSOFT OFFICE 2000(WORD/EXCEL/POWERPOINT)
------------------------------------------------------------

When you scan multiple pages, you cannot change the resolution for each page.
When you want to scan the multiple-page documents using the ADF at a time, please note the following:

The Mixed Original setting should be set to OFF(refer to the operating instructions). The scan size will be fixed to the size you set in the Scan size setting regardless of the original document size.
When, for example, you want to scan both letter-sized documents and legal-sized documents and the Scan size is set to "Legal", all data will be received in legal-size. In this case, it takes more time to scan the documents because white lines will be added to the document length in order to make the letter-sized document into a legal-sized document.  When Scan size is set to "Letter", you will get all letter-sized scan data. In this case, part of the legal-sized documents will be not scanned.

------------------------------------------------------------
FOR THE USERS OF CAERE OMNIPAGE PRO 10.0
------------------------------------------------------------
In order to use the function of this TWAIN Driver fully or use OmniPage Pro without any trouble, please select the following Scan Manager settings in Windows Control Panel:

1. Select "Flatbed Scanner with ADF" in "Device Type" setting.

2. You must select "Yes" in "Show TWAIN settings before scan" setting. 
   Otherwise, you cannot set each scan parameter in the RS mode and you cannot retrieve the image in the SB mode.

3. Select "No" in "Invert black and white images" setting.

4. Select "Yes" in "Support TWAIN batch Scanning" setting.
   Otherwise, only the first page of the documents set in the ADF will be scanned.

------------------------------------------------------------
FOR THE USERS OF SCANSOFT TEXTBRIDGE PRO MILLENNIUM VER.9.5
------------------------------------------------------------
In order to use the function of this TWAIN Driver fully or use the TextBridge without any trouble, please set Scanner Setup of TextBridge as follows:

1. In Scanner Setup of TextBridge, check the check boxes of "Flatbed Scanner" and "with automatic document feeder (ADF)".

2. In Scanner Setup of TextBridge, check the check box of "Show TWAIN Interface".
   Otherwise, only the first page of the documents set in the ADF will be scanned.

3. If you perform the test scan in Scanner Setup of TextBridge, the document must be only one page. Multiple pages cannot be scanned in this case. If you tried to scan multiple pages, the TWAIN Driver cannot be closed. In this case, close TextBridge and the TWAIN Driver using Windows Task Manager.

------------------------------------------------------------
FOR THE USERS OF SCANSOFT PAPERPORT DELUXE 6.5/7.0
------------------------------------------------------------
On the desktop screen of this software, do not click the icon for scanning twice consecutively. Otherwise, the software will freeze. 

------------------------------------------------------------
FOR USERS OF I.R.I.S READIRIS PRO 6
------------------------------------------------------------

If you canceled the scanning job on the TWAIN driver screen and try to open the driver again, "No paper in autofeeder" warning message will be appeared. When you encounter it, select "Cancel" and close the message window, and then open the TWAIN driver again.


******************************************************
V. TRADEMARK NOTICES
******************************************************

Windows, and Microsoft Windows are registered trademarks of Microsoft Corp.

