(Read this file with [Word Wrap] selected in the [Edit] menu of Notepad.
If you are using the version of Notepad included with Windows 2000, Windows XP, Windows Server 2003, Windows Vista, Windows Server 2008, Windows 7, Windows Server 2008 R2, Windows 8, Windows Server 2012, Windows Server 2012 R2, or Windows 10, [Word Wrap] is located in the [Format] menu.)

=================================================================
 "Muratec MFX-1820/2010"                       GDI printer driver

 Copyright (C) MURATA MACHINERY, LTD.
=================================================================
Thank you for purchasing the MFX-1820/2010.
Please make sure to read the following information before installing the software for the machine.

**********************************************************************
    Contents
**********************************************************************
1. Before Installation
   + About This ReadMe File

2. Hardware, Computers, and Supported Operating Systems
   + Hardware
   + Computers
   + Supported Operating Systems

3. General Cautions Regarding Installation

4. Cautions Regarding Printer Driver Installation

5. Printer Driver Cautions / Restrictions

6. Other Cautions / Restrictions

7. Trademarks

**********************************************************************
1. Before Installation
**********************************************************************
Make sure to read this information before installing the software.
----------------------------------------------------------------------
About This ReadMe File
----------------------------------------------------------------------
This file includes cautions, restrictions, and other information regarding the printer drivers for the MFX-1820/2010.


**********************************************************************
2. Hardware, Computers, and Supported Operating Systems
**********************************************************************
----------------------------------------------------------------------
Hardware
----------------------------------------------------------------------
The NP-700 is required to use the printer driver in a network environment.
Confirm that the NP-700 is connected to the MFX-1820/2010.

----------------------------------------------------------------------
Computer
----------------------------------------------------------------------
The software operates on Intel x86/x64 processor based computers in which the following supported operating systems can run.
(For information on the required CPU clock speed and memory, etc., check the recommended system configuration for the operating system.)

[When Using the Software in a Network Environment]
When using the software in a network environment, confirm that the computer has the following network interface:
- 10BASE-T, 100BASE-TX

[When Using the Software with a Local Connection]
When using the software with a local connection, confirm that the computer has the following USB interface:
- USB 2.0 High Speed

----------------------------------------------------------------------
Supported Operating Systems
----------------------------------------------------------------------
The software operates in the following versions of Microsoft Windows:

- Windows(R) 2000
- Windows(R) XP
- Windows(R) XP x64
- Windows Server(R) 2003
- Windows Server(R) 2003 x64
- Windows Vista(R)
- Windows Vista(R) x64
- Windows Server(R) 2008
- Windows Server(R) 2008 x64
- Windows(R) 7
- Windows(R) 7 x64
- Windows Server(R) 2008 R2 x64
- Windows(R) 8
- Windows(R) 8 x64
- Windows Server(R) 2012 x64
- Windows Server(R) 2012 R2 x64
- Windows(R) 10
- Windows(R) 10 x64

* Windows 2000 Professional SP2 or later is supported.

**********************************************************************
3. General Cautions Regarding Installation
**********************************************************************
- When installing the software, close all applications that are running.
- Restart the computer after you install or upgrade the software.
- When installing a new version of the software after deleting the old version, restart the computer after deleting the old version of the software, and then install the new version of the software.
- The software may not be installed correctly if you perform the installation with Power User privileges.
   In such a case, install the software with Administrator privileges.

**********************************************************************
4. Cautions Regarding Printer Driver Installation
**********************************************************************
----------------------------------------------------------------------
Installing a Printer Driver Using the "Standard TCP/IP Port Monitor"
----------------------------------------------------------------------
A Standard TCP/IP Port needs to be installed in order to allow printer drivers to be added using an installer program. (This is usually already installed.)

----------------------------------------------------------------------
Installing a Printer Driver Using the “Standard TCP/IP Port Monitor”
----------------------------------------------------------------------
When installing a printer driver using the “Standard TCP/IP Port Monitor,” it is necessary to use the “Add Standard TCP/IP Printer Port Wizard” to create a new port.
Enter the name or IP address of the Muratec MFP to connect to in [Printer Name or IP Address]. It is recommended that you enter a port name that will enable you to recognize that the port is a printer port in [Port Name] (such as “Printer Port”).
Select [Standard Generic Network Card] for the type of device.

----------------------------------------------------------------------
 “SNMP Status” Setting When Using the “Standard TCP/IP Port Monitor”
----------------------------------------------------------------------
When installing a printer driver using the “Standard TCP/IP Port Monitor,” if you select [SNMP Status Enabled] in [Configure Standard TCP/IP Port Monitor], you can check printer errors (such as when the printer runs out of paper or toner) from the list of printers on the computer or the print queue
If you select [SNMP Status Enabled] in [Standard TCP/IP Port Monitor], confirm that the “SNMP function” is enabled on the Muratec MFP.
If the “SNMP function” is enabled in the “Standard TCP/IP Port Monitor” but disabled on the Muratec MFP, print data will not be output.

If you are using Windows(R) 2000, make sure that [SNMP Status Enabled] is deselected.
If [SNMP Status Enabled] is selected, print data may not be output.


**********************************************************************
5. Printer Driver Cautions / Restrictions
**********************************************************************
-------------------------------------------------------------------------------------------
Changing the Port Number When the Raw Protocol is Set in the “Standard TCP/IP Port Monitor”
-------------------------------------------------------------------------------------------
If Raw is selected as the protocol in the “Standard TCP/IP Port Monitor,” you can change the port number in [Raw Settings] (default value: 9100).
If you change the Raw port number in the “Standard TCP/IP Port Monitor”, also change the port number in [RAW Port (Port 9100)] on the Muratec machine, and set the same value.
If the port number is not set to the same value, you will become unable to print.

The port number in [RAW Port (Port 9100)] can be changed in the Web settings.
For details, refer to the Muratec user’s manual.

----------------------------------------------------------------------
Using the “Sort” Function
----------------------------------------------------------------------
You can specify the Sort function when printing with a Muratec printer driver.
To specify the Sort function, enable [Sort] in the "Destination" tab of the printer driver.
When the above setting is specified, printing may not be performed correctly if you set [Collate] in the printing dialog box of applications such as Microsoft Word.
In such a case, perform printing with [Collate] disabled in the printing dialog box.

----------------------------------------------------------------------
Using the “Enlarge/Reduce/Combine/Booklet Printing” Functions
----------------------------------------------------------------------
When printing is not performed correctly using the “Enlarge/Reduce/Combine/Booklet Printing” functions, set [Document Size] in the properties of the printer driver to the same size as the document.
When printing with the “Enlarge/Reduce” function, the page layout may change or the number of pages may increase or decrease, depending on the document.
In such a case, adjust the page layout in the application, as necessary.

----------------------------------------------------------------------
Using the “Combine” Function
----------------------------------------------------------------------
You can specify the Combine function when printing with a Muratec printer driver.
The Combine function enables you to print multiple pages on a single sheet of paper.
You can specify to print two, four, or eight pages on each sheet.
When printing is performed with the Combine function specified, printing may not be performed correctly if multiple sets are specified to be output in the dialog of the application.
In such a case, perform printing with [Collate] disabled in the printing dialog box.

----------------------------------------------------------------------
When Documents Cannot Be Printed Correctly
----------------------------------------------------------------------
When documents cannot be printed correctly, perform printing with [Enable advanced printing features] disabled in the [Advanced] screen of the printer driver properties.

----------------------------------------------------------------------
When Items Cannot Be Selected in the Printer Driver
----------------------------------------------------------------------
Some functions of combinations cannot be used.
Refer to the Muratec user’s manual and help files for details on each function.

------------------------------------------------------------------------
When Printing Cannot Be Performed Correctly With the Paper Specified in 
When Documents Are Created in Certain Application Software
------------------------------------------------------------------------
Printing may be performed with the paper size and orientation set in application software given priority over the settings in the printer driver, depending on the application software.
Perform printing with the correct settings specified in the application software.

----------------------------------------------------------------------------------
When Documents Created in Certain Application Software Cannot Be Printed Correctly
----------------------------------------------------------------------------------
There may be insufficient memory to perform printing.
If multiple sets are specified to be printed, try printing one set.

----------------------------------------------------------------------
When Using Adobe Acrobat
----------------------------------------------------------------------
When images are not printed correctly, perform printing with [File] > [Print] > [Advanced] > [Print as image] selected in Acrobat.

----------------------------------------------------------------------
When Grouped Documents in Microsoft Excel Cannot Be Printed Correctly
----------------------------------------------------------------------
Check the “Page Setup” in Microsoft Excel and the printer driver settings.
When printing worksheets that have been grouped in Microsoft Excel, each worksheet must have the same page settings and printer driver settings specified.

----------------------------------------------------------------------
Customers Using Microsoft Excel
----------------------------------------------------------------------
When printing is performed using Microsoft Excel, the [Print to File] dialog box may be displayed.
In this case, check whether the printing port is correctly set in the printer properties screen.
If the [Print to File] dialog box is displayed even though the settings are correct, close all the application software you are using and restart the computer.

----------------------------------------------------------------------
Limitations of Microsoft Excel
----------------------------------------------------------------------
If you print using a printer driver other than the one that is set when creating a document in Microsoft Excel, the page layout may change or the position of line breaks inside cells may change, causing data that fit on one page to require two pages.
Also, when you set “Print to 1 x 1 page” in [Scaling] in [Page Setup] in Microsoft Excel, if you change to a printer driver other than the one that is set when creating the document, the zoom ratio may change significantly.
This is due to the way that Microsoft Excel operates.

When you want to print documents created in Microsoft Excel just as they appear in the preview screen using a printer driver, it is necessary to set the same printer driver when creating the document.
When printing multiple sheets in Microsoft Excel at the same time, the second and subsequent sheets may not be printed with the settings specified in the dialog.
In such a case, perform printing with the same page settings specified for each sheet.

----------------------------------------------------------------------
Precautions to take when printing using the "Criss-Cross" function
----------------------------------------------------------------------
The printer will not operate correctly if the "Collate" box is checked in application settings. Uncheck the "Collate" checkbox before printing.


**********************************************************************
6. Other Cautions / Restrictions
**********************************************************************
- When using the energy saving (standby) function of a computer that is using the printer driver with a local connection, re-connect the USB cable after resuming the computer.


**********************************************************************
7. Trademarks
**********************************************************************
Microsoft(R), Windows(R) 2000, Windows(R) XP, Windows Server(R) 2003, Windows Vista(R), Windows Server(R) 2008, Windows(R) 7, Windows Server(R) 2008 R2, Windows(R) 8, Windows Server(R) 2012, Windows Server(R) 2012 R2 and Windows(R) 10 are trademarks or registered trademarks of Microsoft Corporation in the United States and other countries.
Adobe(R), Acrobat(R), and Adobe Systems Incorporated and its subsidiaries are trademarks or registered trademarks in each country.
Intel is a registered trademark of Intel Corporation.
Other product names and company names are trademarks or registered trademarks of their respective companies.
