(Read this file with [Word Wrap] selected in the [Edit] menu of Notepad.
If you are using the version of Notepad included with Windows 2000, Windows XP, Windows Server 2003, Windows Vista, Windows Server 2008, Windows 7, Windows Server 2008 R2, Windows 8, Windows Server 2012, or Windows 10, [Word Wrap] is located in the [Format] menu.)

=====================================================================
 "Muratec Fax"                                 Fax driver
=====================================================================
Thank you for purchasing MFX-2x35.
Please make sure to read the following information before installing the software for the machine.

**********************************************************************
    Contents
**********************************************************************
1. Before Installation
   + About This ReadMe File

2. Computers and Supported Operating Systems
   + Computers
   + Supported Operating Systems

3. General Cautions Regarding Installation

4. Cautions Regarding Fax Driver Installation

5. Fax Driver Cautions / Restrictions

6. Other Cautions / Restrictions

7. Trademarks


**********************************************************************
1. Before Installation
**********************************************************************
Make sure to read this information before installing the software.

----------------------------------------------------------------------
About This ReadMe File
----------------------------------------------------------------------
This file includes cautions, restrictions, and other information regarding the Fax drivers for MFX-2x35.


**********************************************************************
2. Computers and Supported Operating Systems
**********************************************************************
----------------------------------------------------------------------
Computer
----------------------------------------------------------------------
The software operates on Intel x86/x64 processor based computers in which the following supported operating systems can run.
(For information on the required CPU clock speed and memory, etc., check the recommended system configuration for the operating system.)

[When Using the Software in a Network Environment]
When using the software in a network environment, confirm that the computer has the following network interface:
- 10BASE-T, 100BASE-TX

[When Using the Software with a Local Connection]
When using the software with a local connection, confirm that the computer has the following USB interface:
- USB 2.0 High Speed

----------------------------------------------------------------------
Supported Operating Systems
----------------------------------------------------------------------
The software operates in the following versions of Microsoft Windows:

- Windows(R) 2000
- Windows(R) XP
- Windows(R) XP x64
- Windows Server(R) 2003
- Windows Server(R) 2003 x64
- Windows Vista(R)
- Windows Vista(R) x64
- Windows Server(R) 2008
- Windows Server(R) 2008 x64
- Windows(R) 7
- Windows(R) 7 x64
- Windows Server(R) 2008 R2 x64
- Windows(R) 8
- Windows(R) 8 x64
- Windows Server(R) 2012
- Windows(R) 10
- Windows(R) 10 x64

* Windows2000 Professional SP2 or later is supported.


**********************************************************************
3. General Cautions Regarding Installation
**********************************************************************
- When installing the software, close all applications that are running.
- Restart the computer after you install or upgrade the software.
- When installing a new version of the software after deleting the old version, restart the computer 
	after deleting the old version of the software, and then install the new version of the software.
- The software may not be installed correctly if you perform the installation with Power User privileges.
  In such a case, install the software with Administrator privileges.


**********************************************************************
4. Cautions Regarding Fax Driver Installation
**********************************************************************
----------------------------------------------------------------------
Installing the Fax Driver Using the "Standard TCP/IP Port Monitor"
----------------------------------------------------------------------
A Standard TCP/IP Port needs to be installed in order to allow fax drivers to be added using an installer program. (This is usually already installed.)

----------------------------------------------------------------------
Installing the Fax Driver Using the "Standard TCP/IP Port Monitor"
----------------------------------------------------------------------
When installing the fax driver using the "Standard TCP/IP Port Monitor", create a different port to the one created when installing the printer driver.
You can create a new port using the "Add Standard TCP/IP Printer Port Wizard."
Enter the name or IP address of the MFP to connect to in [Printer Name or IP Address]. 
Enter a port name different to the one used when installing the printer driver in [Port Name] (such as "Fax Port").
Select [Standard Generic Network Card] for the type of device.

----------------------------------------------------------------------
"SNMP Status" Setting When Using the "Standard TCP/IP Port Monitor"
----------------------------------------------------------------------
When installing the fax driver using the "Standard TCP/IP Port Monitor", open [Configure Standard TCP/IP Port Monitor] and confirm that [SNMP Status Enabled] is deselected.


**********************************************************************
5. Fax Driver Cautions / Restrictions
**********************************************************************
----------------------------------------------------------------------
Changing the Port Number When the Raw Protocol is Set 
in the "Standard TCP/IP Port Monitor"
----------------------------------------------------------------------
If Raw is selected as the protocol in the "Standard TCP/IP Port Monitor", you can change the port number in [Raw Settings] (default value: 9100).
If you change the Raw port number in the "Standard TCP/IP Port Monitor", also change the port number in [RAW Port (Port 9100)] on the machine, and set the same value.
If the port number is not set to the same value, you will become unable to output from the fax driver.

The port number in [RAW Port (Port 9100)] can be changed in the Web settings.
For details, refer to the user's manual.

----------------------------------------------------------------------------------------
Cautions Regarding Browser Settings When Using the Fax Driver Advanced Mode(Web Browser)
----------------------------------------------------------------------------------------
- When the destination for the fax driver to connect to is included in a proxy, the fax driver may not operate correctly.
 Please don't use the proxy server for the destination address.
- If the security level of the destination for the fax driver to connect to is high, you may not be able to connect.  In this case, register the destination in [Local intranet] or [Trusted Sites] in the browser settings.
- In the advanced mode of the fax driver, various extended functions can be specified using the HTTP protocol.
  When using the advanced mode of the fax driver, specify the time settings and time zone settings for the machine.

----------------------------------------------------------------------
Restrictions on Shared Printer Using Fax Driver (Simple Mode)
----------------------------------------------------------------------
By installing a fax driver (when Simple Mode is selected) as a shared printer on the server, you can use the PC-FAX Send function from a client computer. However, when Windows(R) 2000 is used as the client computer or server, you cannot use the Shared Printer Function that uses the fax driver (Simple Mode).


**********************************************************************
6. Other Cautions / Restrictions
**********************************************************************
Please refer to the user's manual.


**********************************************************************
7. Trademarks
**********************************************************************
Microsoft(R), Windows(R) 2000, Windows(R) XP, Windows Server(R) 2003, Windows Vista(R), Windows Server(R) 2008, Windows(R) 7, Windows Server(R) 2008 R2, Windows(R) 8, Windows Server(R) 2012, and Windows(R) 10 are trademarks or registered trademarks of Microsoft Corporation in the United States and other countries.
Adobe(R), Acrobat(R), and Adobe Systems Incorporated and its subsidiaries are trademarks or registered trademarks in each country.
Intel is a registered trademark of Intel Corporation.
Other product names and company names are trademarks or registered trademarks of their respective companies.


